;File: pwm42cfg.asm

; Author: Eckart Hartmann Date:17/10/2003

; Development progress: Pwm834.df

;

;PwmCfg==========Configure PWM mode:

;C Function prototype: char PwmCfg(char cCfg).

;Description of Function: Select mode and clock source and prescaler.

; User interface: Set parameter1 to the required PWMCON register value.

; Call PwmCfg.

; Returns parameter1.

;Robustness: This function terminates any pulse generation in progress and

; restarts with the new settings.

; Ensure PWPO in CFG842 selects required pins.

;Side effects: None.

;

NAME PWMCFG

$NOMOD51

$IC(..kei842.inc) ; Parameter passing registers for Keil .

$IC(..kei842.dat) ; SFR definition for Keil .

;

public \_PwmCfg

;

?PR?\_PwmCfg?PWMCFG SEGMENT CODE

RSEG ?PR?\_PwmCfg?PWMCFG

\_PwmCfg:

mov PWMCON,cP1l ;Save parameter.

ret

;

;Function End==========================================================Function End

END

;