;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;

; Author : ADI - Apps www.analog.com/MicroConverter

;

; Date : 28 May 1999

;

; File : ADCsingl.asm

;

; Hardware : ADuC812

;

; Description : Performs repeated single ADC conversions and moves

; results to P0 & P2. Sets the red LED on the eval

; board upon completion of each conversion. A new

; conversion is innitiated every 200ms.

; All rate calculations assume an 11.0592MHz Mclk.

;

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

$MOD812 ; Use 8052&ADuC812 predefined symbols

LED EQU P3.4 ; P3.4 drives red LED on eval board

CHAN EQU 0 ; convert this ADC input channel..

; ..chan values can be 0 thru 8

;\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

; BEGINNING OF CODE

CSEG

ORG 0000h

JMP MAIN ; jump to main program

;\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

; INTERRUPT VECTOR SPACE

ORG 0033h ; (ADC ISR)

MOV P0,ADCDATAL ; ADC result low byte to Port0

MOV P2,ADCDATAH ; high nibble and channel ID to Port2

CLR LED ; turn the LED on

RETI

;====================================================================

; MAIN PROGRAM

ORG 004Bh

MAIN:

; PRECONFIGURE...

MOV ADCCON1,#060h ; power up ADC

MOV ADCCON2,#CHAN ; select channel to convert

SETB EA ; enable interrupts

SETB EADC ; enable ADC interrupt

; PERFORM REPEATED SINGLE CONVERSIONS...

AGAIN: SETB LED ; turn the LED off

CALL DELAY ; delay 100ms

SETB SCONV ; innitiate single ADC conversion

; ADC ISR is called upon completion

CALL DELAY ; delay 100ms

JMP AGAIN ; repeat

;\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

; SUBROUTINE

DELAY: ; delay 100ms

MOV R7,#200 ; 200 \* 500us = 100ms

DLY1: MOV R6,#229 ; 229 \* 2.17us = 500us

DJNZ R6,$ ; sit here for 500us

DJNZ R7,DLY1 ; repeat 200 times (100ms total)

RET

;\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

END