;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;

; Author : ADI - Apps www.analog.com/MicroConverter

;

; Date : March 2001

;

; File : pllcon.asm

;

; Hardware : ADuC814

;

; Description : Demonstrates that the CPU can run at different

; speeds determined by the CD bits in the PLLCON SFR.

; 2 to the power of CD (a 3 bit number), is the divider

; ratio that determines the clock frequency at which

; the CPU will run. (CD=0 =>fcore=16.777216MHz,

; CD=7 => fcore=131.072kHz)

;

; The program turns on and off the LED approx every

; 70,000 machine cycles. With the higher frequency

; (CD=0 =>fcore=16.777216MHz) the LED toggles at about

; 10Hz. By pressing the INT0 button the CD bit is

; incremented (CD=1 =>fcore=8.388MHz) and the LED will

; toggle at half the frequency as before. At the

; minimum frequency (CD=7, fcore=131.072kHz) the LED

; toggles at 2.777Hz. By pressing INT0 button again

; CD rolls over to 0 again and the LED

; toggles at 16Hz again.

;

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

$MOD814 ; Use 8052&ADuC814 predefined symbols

LED EQU P3.3 ; P3.3 drives red LED on eval board

;\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

; BEGINNING OF CODE

CSEG

ORG 0000h

JMP MAIN ; jump to main program

;\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

; INTERRUPT VECTOR SPACE

ORG 0003h ; (INT0 ISR)

CPL LED ; complemant LED to indicate INT0

; press.

MOV R2,#136 ; reinitialise R7 and R6 so that

MOV R3,#256 ; after interrupt the full delay

; loop is completed

MOV A, PLLCON ; Only increment CD bits of PLLCON

INC A ; Rollover to PLLCON = xxxxx000b (fmax)

ANL A, #07h ; after PLLCON = xxxxx111b (fmin)

MOV PLLCON, A ; where the x's are 1's and 0's as rqd

RETI

;====================================================================

ORG 0060H ; Start code at address above interrupts

MAIN:

MOV PLLCON, #00H

SETB IT0

SETB EX0 ; enable ext int INT0

; (button on eval board)

SETB EA ; enable interrupts

BLINK: CPL LED

CALL DELAY ; wait for 70,000 machine cycles

; =24ms at fmax

; =3.1875s at fmin

JMP BLINK

;====================================================================

DELAY: ; This loop delays the program for 70,000

; (approx) machine cycles, corresponding

; to a delay of 66ms at fmax and 8.4s

; at fmin

MOV R2,#136 ; 136 \* 256 \* 0.715us = 24ms

DLY1: MOV R3,#256 ;

DJNZ R3,$ ; sit here for 256 x 2 x machine

; cycle time

DJNZ R2,DLY1 ; repeat 136 times (=24ms total @ fmax)

RET

;\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

END