;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;

; Author : ADI - Apps www.analog.com/MicroConverter

;

; Date : 31 Jan 2002

;

; File : ADCpin.asm

;

; Hardware : ADuC831

;

; Description : Performs hardware pin driven ADC conversions and

; outputs results on P0 & P2. Continuously flashes

; LED (independently of ADC routine) at approximately

; 5Hz (assuming an 11.0592MHz Mclk).

;

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

$MOD831 ; Use 8052&ADuC831 predefined symbols

LED EQU P3.4 ; P3.4 drives red LED on eval board

CHAN EQU 0 ; convert this ADC input channel..

; ..chan values can be 0 thru 8

;\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

; BEGINNING OF CODE

CSEG

ORG 0000h

JMP MAIN ; jump to main program

;\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

; INTERRUPT VECTOR SPACE

ORG 0033H ; (ADC ISR)

MOV P0,ADCDATAL ; ADC result low byte to Port0

MOV P2,ADCDATAH ; high nibble and channel ID to Port2

RETI

;====================================================================

; MAIN PROGRAM

ORG 004Bh

MAIN:

; PRECONFIGURE...

MOV ADCCON1,#0B0h ; power up ADC, 12.3us conv+acq time

MOV ADCCON2,#CHAN ; select channel to convert

; LAUNCH CONTINUOUS CONVERSIONS...

SETB EA ; enable interrupts

SETB EADC ; enable ADC interrupt

ORL ADCCON1,#001h ; enable hardware CONVST pin

; CONTINUE WITH OTHER CODE...

AGAIN: CPL LED ; blink (complement) the LED

CALL DELAY ; delay 100ms

JMP AGAIN ; repeat

; the micro is free to continue with other tasks (flashing the LED in

; this case) while the ADC is converting, synchronously to the

; external CONVST pin. results are being handled by the ADC

; interrupt service routine.

;\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

; SUBROUTINE

DELAY: ; delay 100ms

MOV R7,#200 ; 200 \* 500us = 100ms

DLY1: MOV R6,#229 ; 229 \* 2.17us = 500us

DJNZ R6,$ ; sit here for 500us

DJNZ R7,DLY1 ; repeat 200 times (100ms total)

RET

;\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

END