;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;

; Author : ADI - Apps www.analog.com/MicroConverter

;

; Date : March 2001

;

; File : ADCsingl.asm

;

; Hardware : ADuC832

;

; Description : Performs repeated single ADC conversions and moves

; results to UART. Sets the red LED on the eval

; board upon completion of each conversion. A new

; conversion is innitiated every 200ms.

; All rate calculations assume an 2.097152MHz Mclk.

;

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

$MOD832 ; Use 8052&ADuC832 predefined symbols

LED EQU P3.4 ; P3.4 drives red LED on eval board

CHAN EQU 0 ; convert this ADC input channel..

; ..chan values can be 0 thru 6

;\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

; BEGINNING OF CODE

CSEG

ORG 0000h

JMP MAIN ; jump to main program

;\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

ORG 0033H ; INTERRUPT VECTOR SPACE

SETB LED

RETI

;====================================================================

; MAIN PROGRAM

ORG 004Bh

MAIN:

; Set up UART

MOV RCAP2H,#0FFh ; config UART for 9600 baud

MOV RCAP2L,#-7 ;

MOV TH2,#0FFh

MOV TL2,#-7

MOV SCON,#52h

MOV T2CON,#34h

; PRECONFIGURE...

MOV ADCCON1,#080h ; power up ADC

MOV ADCCON2,#CHAN ; select channel to convert

SETB EA ; enable interrupts

SETB EADC ; enable ADC interrupt

; PERFORM REPEATED SINGLE CONVERSIONS...

AGAIN: CLR LED ; turn the LED on

MOV A,#01H ; Delay length

CALL DELAY ; delay 100ms

SETB SCONV ; innitiate single ADC conversion

; ADC ISR is called upon completion

JNB LED,$

MOV A,ADCDATAH

CALL SENDVAL

MOV A,ADCDATAL

CALL SENDVAL

MOV A,#01H ; Delay length

CALL DELAY ; delay 100ms

JMP AGAIN ; repeat

;\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

; SUBROUTINE

DELAY: ; Delays by 100ms \* A

; 100mSec based on 2.097152MHZ

; Core Clock

; i.e. default ADuC812S Clock

MOV R1,A ; Acc holds delay variable

DLY0: MOV R2,#022h ; Set up delay loop0

DLY1: MOV R3,#0FFh ; Set up delay loop1

DJNZ R3,$ ; Dec R3 & Jump here until R3 is 0

DJNZ R2,DLY1 ; Dec R2 & Jump DLY1 until R2 is 0

DJNZ R1,DLY0 ; Dec R1 & Jump DLY0 until R1 is 0

RET ; Return from subroutine

;\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

$INCLUDE(UARTIO.ASM)

END