ADCCONV PAGE 1

1 ;======================================================================

2 ;

3 ; Author : ADI - Apps

4 ;

5 ; Date : 5 November 2001

6 ;

7 ; File : adcconv.asm

8 ;

9 ; Hardware : ADuC834

10 ;

11 ; Description : example routine to continuosuly trigger

12 ; a single conversion on the ADC main channel

13 ; The Conversion result is written to external memory,

14 ; P3.4 is toggled 5 times at 100ms delay

15 ; The ADC result is written to external memory

16 ; P3.4 is toggled 5 times at 500ms

17 ; and the sequence repeats itself.

18 ;

19 ;======================================================================

20 ;

21 $MOD834 ; Use 8052&ADuC834 predefined symbols

22

0000 23 FLAG EQU 00H ; Define Bit

24

25

---- 26 CSEG ; Defines the following as a segment of code

27

0000 28 ORG 0000H ; Load Code at '0'

29

0000 020060 30 JMP START ; Jump to START

31 ;

32 ;======================================================================

33 ;

0033 34 ORG 0033H ; Read ADC Result H/M/L to external Memory

35

36 ; 10 flashes at 100ms

0033 7401 37 MOV A,#01H ; 100msec delay

0035 7B0A 38 MOV R3,#0Ah ; loop=5

0037 B2B4 39 TIC1: CPL P3.4 ; Toggle LED

0039 120079 40 CALL DELAY ; Delay 100mSec

003C DBF9 41 DJNZ R3,TIC1 ; Dec loop

42

003E 900000 43 MOV DPTR, #00H ; DPTR=00

0041 E5D9 44 MOV A,ADC0L ; read ADC low byte

0043 F0 45 MOVX @DPTR,A ; write low byte to ext memory

0044 A3 46 INC DPTR ; DPTR=01

0045 E5DA 47 MOV A,ADC0M ; read ADC Middle byte

0047 F0 48 MOVX @DPTR,A ; write Middle byte to ext memory

0048 A3 49 INC DPTR ; DPTR=02

0049 E5DB 50 MOV A,ADC0H ; read ADC High byte

004B F0 51 MOVX @DPTR,A ; write low High byte to ext memory

004C A3 52 INC DPTR

53

54 ; 5 flashes at 500ms

004D 7405 55 MOV A,#05H ; 500msec delay

004F 7B0A 56 MOV R3,#0Ah ; loop=10

0051 B2B4 57 TIC2: CPL P3.4 ; Toggle LED

0053 120079 58 CALL Delay ; Delay 100mSec

ADCCONV PAGE 2

0056 DBF9 59 DJNZ R3,TIC2 ; Dec loop

60 ;

0058 D200 61 SETB Flag ; Set Flag

62

005A 32 63 RETI ; Return from Interrupt

64 ;

65 ;======================================================================

66 ;

0060 67 ORG 0060H

0060 68 START:

69 ; Configure Interrupt System

0060 D288 70 SETB IT0 ; CONFIG EXTERNAL INTERRUPT Falling Edge

0062 D2AF 71 SETB EA ; Enable Global Interrupts

72

73 ; Configure ADC

0064 75D120 74 MOV ADCMODE,#20H ; ENABLE MAIN ADC; Mode- Power down

0067 75D240 75 MOV ADC0CON,#40H ; 24 BITS

76 ; USE EXTERNAL REFERENCE

77 ; AIN1-AIN2

78 ; BIPOLAR MODE

79 ; RANGE = +/-20mV

006A D2AE 80 SETB EADC ; ENABLE ADC INTERRUPT

81

82 ; Looped single conversions

006C C200 83 CONV: CLR FLAG ; Initial condition for FLAG variable

006E 75D122 84 MOV ADCMODE,#22H ; INITIATE A MAIN ADC SINGLE CONVERSION

0071 120079 85 CALL DELAY ; Jump to subroutine DELAY

0074 3000FD 86 JNB FLAG,$ ; Stay here until FLAG=1 i.e. wait for ADC Int.

0077 80F3 87 JMP CONV ; Next ADC Conversion

88 ;

89 ;======================================================================

90 ;

91

0079 92 DELAY: ; Delays by A\*100ms (default Core Clk =1.57MHz)

0079 F8 93 MOV R0,A ; Acc holds delay variable

007A 79FE 94 DLY0: MOV R1,#0FEh ; Set up delay loop0

007C 7A19 95 DLY1: MOV R2,#019h ; Set up delay loop1

007E DAFE 96 DJNZ R2,$ ; Dec R2 & Jump here until R2 is 0

0080 D9FA 97 DJNZ R1,DLY1 ; Dec R1 & Jump DLY1 until R1 is 0

0082 D8F6 98 DJNZ R0,DLY0 ; Dec R0 & Jump DLY0 until R0 is 0

0084 22 99 RET ; Return from subroutine

100 ;

101 END

102

103

104

VERSION 1.2h ASSEMBLY COMPLETE, 0 ERRORS FOUND

ADCCONV PAGE 3

ADC0CON. . . . . . . . . . . . . D ADDR 00D2H PREDEFINED

ADC0H. . . . . . . . . . . . . . D ADDR 00DBH PREDEFINED

ADC0L. . . . . . . . . . . . . . D ADDR 00D9H PREDEFINED

ADC0M. . . . . . . . . . . . . . D ADDR 00DAH PREDEFINED

ADCMODE. . . . . . . . . . . . . D ADDR 00D1H PREDEFINED

CONV . . . . . . . . . . . . . . C ADDR 006CH

DELAY. . . . . . . . . . . . . . C ADDR 0079H

DLY0 . . . . . . . . . . . . . . C ADDR 007AH

DLY1 . . . . . . . . . . . . . . C ADDR 007CH

EA . . . . . . . . . . . . . . . B ADDR 00AFH PREDEFINED

EADC . . . . . . . . . . . . . . B ADDR 00AEH PREDEFINED

FLAG . . . . . . . . . . . . . . NUMB 0000H

IT0. . . . . . . . . . . . . . . B ADDR 0088H PREDEFINED

P3 . . . . . . . . . . . . . . . D ADDR 00B0H PREDEFINED

START. . . . . . . . . . . . . . C ADDR 0060H

TIC1 . . . . . . . . . . . . . . C ADDR 0037H

TIC2 . . . . . . . . . . . . . . C ADDR 0051H