;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;

; Author : ADI - Apps www.analog.com/MicroConverter

;

; Date : 5 November 2001

;

; File : DualDPTR.asm

;

; Hardware : ADuC836

;

; Description : Sample Program to show the new ADuC836 features

; of dual DPTRs.

;

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

$MOD836 ; Use 8052&ADuC836 predefined symbols

LED EQU P3.4 ; P3.4 drives red LED on eval board

;\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

; BEGINNING OF CODE

CSEG

ORG 0000h

; highest speed

MOV PLLCON, #0

; CONFIGURE UART....

MOV T3CON,#85h

MOV T3FD,#12h

MOV SCON,#52h

; enable the intenal On-Chip XRAM

MOV CFG836, #01h

; move 512 bytes from code memory (adress 1000h -> 1200h) into

; data XRAM (address 0000h -> 0200h)

; configure the datapointer

MOV DPTR, #0

MOV DPCON, #55h ; auto toggle between DPTRs

; auto increment shadow DPTR

; auto increment main DPTR

; select shadow DPTR

MOV DPTR, #1000h

COPYDATALOOP:

; read Code Memory using Shadow DPTR

CLR A

MOVC A, @A+DPTR ; read code memory

; auto increment shadow DPTR

; swap to main DPTR

; write to XRAM using main DPTR

MOVX @DPTR, A ; write to XRAM

; auto increment main DPTR

; swap to shadow DPTR

; check if at end of loop

; NOTE: shadow DPTR selected (not main)

MOV A, DPH

CJNE A, #12h, COPYDATALOOP

NOP ; <----NOTE: Set a breakpoint in the debugger here

; This will show that the values in code memory

; at addresses 1000h thru 1200h has been mapped

; into XRAM at address 0000h thru 0200h.

; The debugger will not run the nextpiece of

; code as this requires the use of the serial port

; transmit XRAM up UART

MOV DPCON, #4 ; select main DPTR

; auto increment DPTR

; do not toggle DPTR

MOV DPTR, #0

MOV R0, #16

SENDXRAM:

MOVX A, @DPTR

CALL SENDVAL

DJNZ R0, SENDXRAM

; send a newline

MOV A, #10

CALL SENDCHAR

MOV A, #13

CALL SENDCHAR

MOV R0, #16

MOV A, DPH

CJNE A, #2, SENDXRAM

JMP $

;\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

; SENDVAL

SENDVAL: ; converts the hex value of A into two ASCII chars,

; and then spits these two characters up the UART.

; does not change the value of A.

PUSH ACC

SWAP A

CALL HEX2ASCII

CALL SENDCHAR ; send high nibble

POP ACC

PUSH ACC

CALL HEX2ASCII

CALL SENDCHAR ; send low nibble

POP ACC

RET

;\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

; SENDCHAR

SENDCHAR: ; sends ASCII value contained in A to UART

JNB TI,$ ; wait til present char gone

CLR TI ; must clear TI

MOV SBUF,A

RET

;\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

; HEX2ASCII

HEX2ASCII: ; converts A into the hex character representing the

; value of A's least significant nibble

ANL A,#00Fh

CJNE A,#00Ah,$+3

JC IO0030

ADD A,#007h

IO0030: ADD A,#'0'

RET

;\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

ORG 1000h

DB 00h,01h,02h,03h,04h,05h,06h,07h,08h,09h,0Ah,0Bh,0Ch,0Dh,0Eh,0Fh

DB 10h,11h,12h,13h,14h,15h,16h,17h,18h,19h,1Ah,1Bh,1Ch,1Dh,1Eh,1Fh

DB 20h,21h,22h,23h,24h,25h,26h,27h,28h,29h,2Ah,2Bh,2Ch,2Dh,2Eh,2Fh

DB 30h,31h,32h,33h,34h,35h,36h,37h,38h,39h,3Ah,3Bh,3Ch,3Dh,3Eh,3Fh

DB 00h,01h,02h,03h,04h,05h,06h,07h,08h,09h,0Ah,0Bh,0Ch,0Dh,0Eh,0Fh

DB 10h,11h,12h,13h,14h,15h,16h,17h,18h,19h,1Ah,1Bh,1Ch,1Dh,1Eh,1Fh

DB 20h,21h,22h,23h,24h,25h,26h,27h,28h,29h,2Ah,2Bh,2Ch,2Dh,2Eh,2Fh

DB 30h,31h,32h,33h,34h,35h,36h,37h,38h,39h,3Ah,3Bh,3Ch,3Dh,3Eh,3Fh

DB 00h,01h,02h,03h,04h,05h,06h,07h,08h,09h,0Ah,0Bh,0Ch,0Dh,0Eh,0Fh

DB 10h,11h,12h,13h,14h,15h,16h,17h,18h,19h,1Ah,1Bh,1Ch,1Dh,1Eh,1Fh

DB 20h,21h,22h,23h,24h,25h,26h,27h,28h,29h,2Ah,2Bh,2Ch,2Dh,2Eh,2Fh

DB 30h,31h,32h,33h,34h,35h,36h,37h,38h,39h,3Ah,3Bh,3Ch,3Dh,3Eh,3Fh

DB 00h,01h,02h,03h,04h,05h,06h,07h,08h,09h,0Ah,0Bh,0Ch,0Dh,0Eh,0Fh

DB 10h,11h,12h,13h,14h,15h,16h,17h,18h,19h,1Ah,1Bh,1Ch,1Dh,1Eh,1Fh

DB 20h,21h,22h,23h,24h,25h,26h,27h,28h,29h,2Ah,2Bh,2Ch,2Dh,2Eh,2Fh

DB 30h,31h,32h,33h,34h,35h,36h,37h,38h,39h,3Ah,3Bh,3Ch,3Dh,3Eh,3Fh

DB 00h,01h,02h,03h,04h,05h,06h,07h,08h,09h,0Ah,0Bh,0Ch,0Dh,0Eh,0Fh

DB 10h,11h,12h,13h,14h,15h,16h,17h,18h,19h,1Ah,1Bh,1Ch,1Dh,1Eh,1Fh

DB 20h,21h,22h,23h,24h,25h,26h,27h,28h,29h,2Ah,2Bh,2Ch,2Dh,2Eh,2Fh

DB 30h,31h,32h,33h,34h,35h,36h,37h,38h,39h,3Ah,3Bh,3Ch,3Dh,3Eh,3Fh

DB 00h,01h,02h,03h,04h,05h,06h,07h,08h,09h,0Ah,0Bh,0Ch,0Dh,0Eh,0Fh

DB 10h,11h,12h,13h,14h,15h,16h,17h,18h,19h,1Ah,1Bh,1Ch,1Dh,1Eh,1Fh

DB 20h,21h,22h,23h,24h,25h,26h,27h,28h,29h,2Ah,2Bh,2Ch,2Dh,2Eh,2Fh

DB 30h,31h,32h,33h,34h,35h,36h,37h,38h,39h,3Ah,3Bh,3Ch,3Dh,3Eh,3Fh

DB 00h,01h,02h,03h,04h,05h,06h,07h,08h,09h,0Ah,0Bh,0Ch,0Dh,0Eh,0Fh

DB 10h,11h,12h,13h,14h,15h,16h,17h,18h,19h,1Ah,1Bh,1Ch,1Dh,1Eh,1Fh

DB 20h,21h,22h,23h,24h,25h,26h,27h,28h,29h,2Ah,2Bh,2Ch,2Dh,2Eh,2Fh

DB 30h,31h,32h,33h,34h,35h,36h,37h,38h,39h,3Ah,3Bh,3Ch,3Dh,3Eh,3Fh

DB 00h,01h,02h,03h,04h,05h,06h,07h,08h,09h,0Ah,0Bh,0Ch,0Dh,0Eh,0Fh

DB 10h,11h,12h,13h,14h,15h,16h,17h,18h,19h,1Ah,1Bh,1Ch,1Dh,1Eh,1Fh

DB 20h,21h,22h,23h,24h,25h,26h,27h,28h,29h,2Ah,2Bh,2Ch,2Dh,2Eh,2Fh

DB 30h,31h,32h,33h,34h,35h,36h,37h,38h,39h,3Ah,3Bh,3Ch,3Dh,3Eh,3Fh

;\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

END