;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;

; Author : ADI - Apps www.analog.com/MicroConverter

;

; Date : October 2003

;

; File : ADCsingl.asm

;

; Hardware : ADuC841

;

; Description : Performs repeated single ADC conversions and moves

; results to P0 & P2. Sets the red LED on the eval

; board upon completion of each conversion. A new

; conversion is innitiated every 200ms.

; All rate calculations assume an 11.0592MHz Mclk.

;

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

$MOD841 ; Use 8052&ADuC841 predefined symbols

LED EQU P3.4 ; P3.4 drives red LED on eval board

CHAN EQU 0 ; convert this ADC input channel..

; ..chan values can be 0 thru 8

;\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

; BEGINNING OF CODE

CSEG

ORG 0000h

JMP MAIN ; jump to main program

;\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

; INTERRUPT VECTOR SPACE

ORG 0033h ; (ADC ISR)

MOV P0,ADCDATAL ; ADC result low byte to Port0

MOV P2,ADCDATAH ; high nibble and channel ID to Port2

CLR LED ; turn LED on

RETI

;====================================================================

; MAIN PROGRAM

ORG 004Bh

MAIN:

; PRECONFIGURE...

MOV ADCCON1,#09Ch ; power up ADC ADCLK = MCLK/4

MOV ADCCON2,#CHAN ; select channel to convert

SETB EA ; enable interrupts

SETB EADC ; enable ADC interrupt

; PERFORM REPEATED SINGLE CONVERSIONS...

MOV A,#010 ; set delay length

AGAIN: SETB LED ; turn the LED off

CALL DELAY ; delay 100mS

SETB SCONV ; innitiate single ADC conversion

; ADC ISR is called upon completion

CALL DELAY ; delay 100ms

JMP AGAIN ; repeat

;\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

; SUBROUTINE

DELAY: ; delay 10ms X A

MOV R5,A

DLY2: MOV R7,#090h

DLY1: MOV R6,#0FFh

DJNZ R6,$

DJNZ R7,DLY1

DJNZ R5,DLY2

RET

;\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

END