;======================================================================

;

; Author : ADI - Apps

;

; Date : 31st Oct 2003

;

; Filename : INT0BLNK.ASM

;

; Hardware : ADuC847

;

; Description : Blinks LED continuously.

; with 50% duty cycle.

; Pressing Int0 slows LED toggle rate

;

;======================================================================

;

$MOD847 ; Use ADuC847 predefined Symbols

LED EQU P3.4 ; P3.4 is red LED on eval board

FLAG BIT 00H ; define Flag variable

CSEG ; Defines the following as a segment of code

ORG 0000H ; Load Code at '00H'

JMP MAIN ; Jump to MAIN

;======================================================================

ORG 0003h ; (INT0 ISR)

INC A ; Increment Acc

RETI ; Return from Interrupt

;======================================================================

; Subroutines

;------------------------------------------------------------------

DELAY:

MOV R0,A ; Acc holds delay variable

DLY0: MOV R1,#0C8h ; Set up delay loop0

DLY1: MOV R2,#0C8h ; Set up delay loop1

DJNZ R2,$ ; Dec R2 & Jump here until R2 is 0

DJNZ R1,DLY1 ; Dec R1 & Jump DLY1 until R1 is 0

DJNZ R0,DLY0 ; Dec R0 & Jump DLY0 until R0 is 0

RET ; Return from subroutine

;======================================================================

MAIN: ; (main program)

SETB IT0 ; INT0 edge triggered

SETB EA ; enable inturrupts

SETB EX0 ; enable INT0

CLR FLAG ; Clear Bit defined as FLAG

MOV A,#02H ; Initialize A -> 1

BLINK: CPL LED ; blink LED using compliment instruction

CALL DELAY ; Jump to subroutine DELAY

JNB FLAG,BLINK ; If FLAG is still cleared the jump to Blink

END