This Boost Converter example application can be used to control the high-power

LED module of an Infineon EasyKit XC822.

The touchpads have the following function:

TP1: Increase brightness of LED module

TP2: ON/OFF LED module

TP3: Reduce brightness of LED module

This application is configured for the on-chip flash of the XC822 controller.

It must be downloaded before testing or debugging.

For more information, please refer to the Infineon Getting Started manual

for the EasyKit XC822 board.