The BLINKY program is a very simple program that blinks the LED's on

connected to Port 5 of the MCB950. When you can successfully build

and run this program, you have used the entire toolset including:

The uVision integrated development environment.

The C51 compiler, linker and the uVision simulator/debugger.

This BLINKY program is available in several targets:

Simulator: for uVision Debugger testing with simulator

ULINK2 NXP 95x: for Debugging with Keil ULINK2 JTAG adapter

FS2 System Navigtor: for Debugging with the FS2 System Navigator

Use the following jumper settings on the MCB900 board:

RUN: OFF RESET: ON for Download with Flash Magic

RUN: ON RESET: OFF for Program Run