The AD4INPUT program reads the four input pairs AIN0-AIN1,

AIN2-AIN3, AIN4-IN5, AIN6-AIN7 of the MSC121x and outputs

the values along with other A/D relevant information via

the serial interface.

This example shows a simple method to convert the A/D HEX

values into a voltage value that is more readable. The

algorithm uses only long arithmetic and avoids any loss of

precision as it would be the case when using single precision

floating point arithmetic.

Also shown is the usage of the uVision simulator. The file

Debugger.INI defines a signal function that creates a voltage

ramp on AIN0-AIN1. Toolbox buttons are defined for easy access

to this signal function. The other analog inputs are set to

random input voltages.

The example is available in three targets:

ISD51 - EVM - 22.1184MHz:

generates the program for the TI MSC1200EVM board that uses an

22.1184MHz XTAL. It can be debugged using the ISD51 In-System

Debugger with 19200bps communication baudrate.

Simulator:

generates the program for running without ISD51 (at 22.1184MHz)

or for testing with the uVision Simulator.