The sub-folders contain pre-configured Monitor versions for various

Atmel 8051 device variants.

Currently the following Devices are configured.

AT89C5131: use Monitor in folder T89C51RC2

AT89C5132: use Monitor in folder AT89C51SND1

AT89C51CC03: use Monitor in folder AT89C51CC03

AT89C51RD2: use Monitor in folder AT89C51RD2

AT89C51SND1: use Monitor in folder AT89C51SND1

AT89C51SND2: use Monitor in folder AT89C51SND1

T89C51AC2: use Monitor in folder T89C51CC01

T89C51CC01: use Monitor in folder T89C51CC01

AT89C51RD2: use Monitor in folder AT89C51RD2