How to load the Monitor into the Systronix uCAN2:

=================================================

The µCAN2 has an integrated loader, that is able to load

the MON390 to RAM. To perform this load, you have to:

- Connect the board to the PC via the uCAN2 COM1 serial port.

- Open a standard windows terminal emulation, like 'Hyperterminal'.

- Activate the loader on uCAN2, by pressing the LOAD button.

- Type Enter (CR) in the terminal emulation. This displays:

Unified HSM HEX LOADER & DEMONSTRATOR Rev xxx

(C)1996-1999 SYSTRONIX, INC.

Type '?' for command help

uCAN2/prog:00>

- Type 'L' and select the file sending option of your terminal emulation.

Select the file Keil\C51\MON390\Systronix uCAN2 Monitor\MON390.HEX and

send it to the board.

- Now you reset the board, to start the MON390.