MONITOR-51 Version 2.9 Release Note:

====================================

Since version 2.8 the MONITOR 51 can be installed on DALLAS 80C320/520/530

target systems. Previous versions were not able to handle multiple DPTR

register and crashed when a different DPTR was selected.

Please use serial type 4, 5, 11 or 12 during installation when a DALLAS

microcontroller should be used.

Since version 2.9 the MONITOR 51 can execute some code before and after

a go and procedure step command. This might be used for changing the memory

layout or changing the serial transmission parameters.

In order to do this, you can insert some code after the BEFORE\_GO and AFTER\_GO

labels in the INSTALL.A51 configuration file.