This example demonstrates bank switching with the Mentor M8051EW

Memory Extension. It uses the IBANKING linker/locater directive.

The example is available in two targets:

LX51: for the extended LX51 Linker/Locater

BL51: for the standard BL51 Linker/Locater