The ISD51\_Demo project for the Philips LPC952 shows how to use the

ISD51 In-System-Debugger with flash breakpoints.

This example just blinks with one LED on the Keil MCB950 evaluation

board and echoes all characters on the serial interface.