Special Notes on the MON390 for DALLAS5240:

===========================================

Limitations:

- The Monitor uses the RAM1 area for XDATA. The extended stack

cannot be enabled with the monitor.

- The Monitor will \*not work\* in the 128KB DS5002 compatiblity mode.