This example program uses RTX51 Tiny to control 4 tasks and to

pass signals between the tasks. The tasks in this program do

nothing more than increment counters and delay for a few clock ticks.